[general]
name=Shape Tools
qgisMinimumVersion=3.4
description=Shape Tools is a collection of geodesic shapes and tools. Create circle, ellipse, line of bearing, points along a line of bearing, concentric circles, pie wedge, donut, arc wedge, star, ellipse rose, epicycloid, gear, hypocyloid, polyfoil, polygon, radial line, rings with radial lines, and heart shapes. Tools include "XY to Line" tool, densify lines and polygons along geodesic paths, geodesic line break, geodesic measuring and create a measurement layer, geodesic scale, rotate, flip and translate tools, and digitize points at an azimuth & distance tools.
version=3.4.19
author=C Hamilton
email=adenaculture@gmail.com
about=Shape Tools is a collection of geodesic shapes and tools. Shape Tools is installed in the Vector menu.
    "Create Geodesic Shapes" processes a point vector layer to create circles, ellipses, arc wedges, pie wedges, donuts, lines of bearing, points along a line of bearing, ellipse roses, epicycloids, hypocyloids, polyfoils, polygons, radial lines, rings with radial lines, stars, and hearts based on the table's fields and other parameters.
    "Interactive Geodesic Shapes" captures the coordinate of a mouse click on the canvas and draws the selected shape about it.
    "XY to Line" uses pairs of coordinates from each record to create geodesic lines. 
    "Geodesic Line Break" breaks lines at the International Date Line. 
    "Geodesic Densifier" creates geodesic lines and polygons by adding additional vertices along geodesic paths within the shape. 
    "Geodesic distance & Time Decimation" remove points or vertices from a point or line layer using geodesic distances or time.
    "Geodesic Measure Tool" measures distances using the WGS 84 ellipsoid and includes the bearing or heading between points. It will even saves the measurements as a layer.
    "Geodesic Measurement Layer" converts a polygon or line layer a new layer with all geometries measured and labeled.
    "Geodesic Transformation Tool" can scale, rotate and translate any shape.
    "Geodesic flip & rotate tools" provide geodesic flip and rotation vector feature transformations.
    "Azimuth, Distance Digitizer" digitizes points based on a clicked point, an azimuth and distance or creates a geodesic line from a clicked point to an azimuth and distance.
    "Field Calculator Functions" provides geodesic functions in the field calculator.
tracker=https://github.com/NationalSecurityAgency/qgis-shapetools-plugin/issues
repository=https://github.com/NationalSecurityAgency/qgis-shapetools-plugin
tags=ellipse,pie,circle,donut,bearing,gear,polygon,star,rose,hypocyloid,polyfoil,epicycloid,heart,xy to line,geodesic line,geodesic polygon,densifier,densify,decimate,decimation,simplify,measure,measurements,azimuth,distance,digitize,line split,international date line,surveying,resize,scale,rotate,flip,translate,expression,field calculator,concentric,circles
homepage=https://github.com/NationalSecurityAgency/qgis-shapetools-plugin
category=Vector
icon=icon.png
experimental=False
deprecated=False
hasProcessingProvider=yes
changelog=
    3.4.19 - Fix bug in Create radial lines
    3.4.18 - Add license to output plugin.
    3.4.17 - Fix bug in geodesic densify algorithm
    3.4.16 - Add rings with radial lines shape
    3.4.15 - Add interactive donut and concentric circles with radial lines algorithms.
    3.4.14 - Add create circle algorithm
    3.4.13 - Geodesic measure layer can add compass directions to label.
    3.4.12 - Fix to allow qgis_process to function correctly.
    3.4.11 - Add st_compass(...) expression.
    3.4.10 - Add compass cardinal directions to geodesic measurements
    3.4.9 - Update translation
    3.4.8 - Add a shape that looks like a gear
    3.4.7 - Updated translation
    3.4.6 - Added a point along a line of bearing algorithm and offset to line of bearing algorithm.
    3.4.5 - Changed the geodesic measure tool to not add a final end point with right click, but simply stop measuring.
    3.4.4 - Add a settings icon to the geodesic measure tool.
    3.4.3 - Made geodesic measture tool's unit of measure persistent.
    3.4.2 - Address feature request #42
    3.4.1 - Add an option for the measurement layer to include original attributes.
    3.4.0 - Added field calculator functions.
    3.3.19 - Rewrote geodesic creation algorithms to include data defined overrides.
    3.3.18 - Added data defined overrides to the geodesic transformations algorithm.
    3.3.17 - Addressed issues #37 and #38.
    3.3.16 - Arc wedge now creates a donut if a full 360 degrees are specified.
    3.3.15 - Replace PNG icons with SVG icons and resize other PNG icons.
    3.3.14 - Added geodesic measure tool save to layer significant digits.
    3.3.13 - Force shape creation to 0-360 degree range when crossing the -180/180 boundary
    3.3.12 - Add radial lines shape
    3.3.11 - Bug fix in settings
    3.3.10 - Added geodesic decimation and time decimation.
    3.3.9 - Snapping enabled in Azimuth Distance Digitizers.
    3.3.8 - Snapping was added to geodesic measurement tool.
    3.3.7 - Added exact coordinate entry in measurement tool.
    3.3.6 - Added Chinese language support
    3.3.5 - Added the ability to quickly copy geodesic measurement values onto the clipboard.
